1. Contact FAA and report flight
2. Put on Latex gloves
3. Set up tarp and lay out materials
4. Final Test of Software (Writing to USB)
5. Replace all resistors
6. Replace all batteries
7. Load Spring
8. Fold & Insert Parachutes
9. Inflate Balloon & Tie closed
10. Attach Balloon to weight
11. Plug in MyRio - check lights for proper status
12. Arm burn-switch
13. Final Sealing of hardware case – include crash wadding
14. Connect MyRio to balloon
15. Disconnect Ballloon from weight